Compliance Statement for the Restriction of Hazardous Substances (RoHS)
Restriction of Hazardous Substances in Electrical and Electronic Equipment
References
1. Directive 2011/65/EU (RoHS 2)
2. Commission Delegated Directive (EU) 2015/863 (RoHS 3)
Restricted Substances
The following substances are restricted under Directive 2011/65/EU, as amended by Directive (EU) 2015/863. The maximum concentration values permitted in homogeneous materials are shown below.
	Substance
	Maximum Concentration

	Lead (Pb)
	0.1% (1000 ppm)

	Mercury (Hg)
	0.1% (1000 ppm)

	Cadmium (Cd)
	0.01% (100 ppm)

	Hexavalent Chromium (Cr⁶⁺)
	0.1% (1000 ppm)

	Polybrominated Biphenyls (PBB)
	0.1% (1000 ppm)

	Polybrominated Diphenyl Ethers (PBDE)
	0.1% (1000 ppm)

	Bis(2-ethylhexyl) Phthalate (DEHP)
	0.1% (1000 ppm)

	Benzyl Butyl Phthalate (BBP)
	0.1% (1000 ppm)

	Dibutyl Phthalate (DBP)
	0.1% (1000 ppm)

	Diisobutyl Phthalate (DIBP)
	0.1% (1000 ppm)


Statement of Compliance
Products manufactured by Halsit Holdings, LLC dba Abbatron are, to the best of our knowledge and based upon information provided by our suppliers, compliant with Directive 2011/65/EU and its amendments, including Commission Delegated Directive (EU) 2015/863.

Compliance is achieved through material composition meeting the applicable RoHS substance restrictions or through the use of valid exemptions permitted under the Directive.
RoHS Exemption Declaration
Certain products may contain materials that utilize allowable exemptions under Directive 2011/65/EU and its amendments where technically necessary.
Exemption 6(a): Lead as an alloying element in steel.
Exemption 6(c): Copper alloy containing up to 4% lead by weight.
Applicable exemptions are used only where permitted under the current RoHS Directive and its amendments.

Abbatron does not maintain part-level material declarations or Full Material Declarations (FMDs) unless specifically required by contract or customer agreement.
Document Revision Date
July 2026

James A. Sitter
President
